Expire: October, 1998 [Page 1]

Network Working Group                                       P. Johansson
Internet-Draft                                  Congruent Software, Inc.
<draft-ietf-ip1394-mcap-00.txt>
Expires: October, 1998

       Multicast Channel Allocation Protocol (MCAP) for IEEE 1394

STATUS OF THIS DOCUMENT

This document is an Internet-Draft. Internet-Drafts are working
documents of the Internet Engineering Task Force (IETF), its areas, and
its working groups. Note that other groups may also distribute working
documents as Internet-Drafts.

Internet-Drafts are draft documents valid for a maximum of six months
and may be updated, replaced, or obsoleted by other documents at any
time. It is inappropriate to use Internet-Drafts as reference material
or to cite them other than as "work in progress."

To view the entire list of current Internet-Drafts, please check the
"1id-abstracts.txt" listing contained in the Internet-Drafts Shadow
Directories on ftp.is.co.za (Africa), ftp.nordu.net (Europe),
munnari.oz.au (Pacific Rim), ds.internic.net (US East Coast), or
ftp.isi.edu (US West Coast).

ABSTRACT

This document specifies how IP-capable Serial Bus devices may allocate
IEEE 1394 channel number(s) for use in the multicast transmission of IP
datagrams. It defines the necessary methods, data structures and codes
for that purpose.

See also the most recent revision of draft-ietf-ip1394-ipv4 for a
specification of the transport of IPv4 datagrams over IEEE 1394.

CAUTION: This is a WORKING DOCUMENT of the IETF IP/1394 group; some
parts reflect rough consensus achieved at the 41st IETF meeting in Los
Angeles, other parts reflect the editor’s distillation of comments on
the reflector since then and still other parts are new contributions to
the evolution of MCAP. Until subsequent revisions of this document are
posted that more clearly identify agreed areas, the reader should
consider this a work in progress very much subject to revision. This
document is not yet adopted by the IP/1394 working group.

Internet-Draft 00 1394 MCAP April 1998

TABLE OF CONTENTS

1. INTRODUCTION ....................................................... 3

2. DEFINITIONS AND NOTATION ........................................... 3

   2.1 Conformance .................................................... 3

   2.2 Glossary ....................................................... 4

   2.3 Abbreviations .................................................. 4

3. CHANNEL ALLOCATION MANAGER ......................................... 5

4. MCAP MESSAGE FORMAT ................................................ 5

5. MCAP OPERATIONS .................................................... 8

   5.1 Advertisement of channel mappings .............................. 8

   5.2 Request for channel allocation ................................. 8

   5.3 Error response to channel allocation ........................... 9

   5.4 Release of unneeded channel(s) ................................ 10

   5.5 Solicitation of the channel map ............................... 10

   5.6 Periodic refresh of channel allocation(s) ..................... 11

6. SECURITY CONSIDERATIONS ........................................... 11

7. ACKNOWLEDGEMENTS .................................................. 11

8. REFERENCES ........................................................ 11

9. EDITOR�S ADDRESS .................................................. 12

Internet-Draft 00 1394 MCAP April 1998

1. INTRODUCTION

This document specifies how IP-capable Serial Bus devices may allocate
IEEE 1394 channel number(s) for use in the multicast transmission of IP
datagrams. It defines the necessary methods, data structures and codes
for that purpose.

The group of IEEE standards and supplements, draft or approved, related
to IEEE Std 1394-1995 is hereafter referred to either as 1394 or as
Serial Bus.

The draft specification for the transport of IPv4 datagrams over 1394,
draft-ietf-ip1394-ipv4, requires broadcast and multicast IP datagrams to
be transported within 1394 asynchronous streams. Before an asynchronous
stream may be used it is necessary to allocate a 1394 resource, a
channel number. The IPv4 draft specification describes how a channel
number is allocated for all broadcast IP datagrams; this same channel
number is also used, by default, for multicast traffic.

In cases where it is desirable to use a different channel number for
particular multicast groups, methods are needed to allocate a channel
number, advertise its existence and ultimately deallocate the channel
number when it is no longer needed. This document describes such methods
and names them "multicast channel allocation protocol" (MCAP).

Although the definition of MCAP is motivated by the particular
requirements of 1394, the methods are extensible to other link media.

CAUTION: This is a WORKING DOCUMENT of the IETF IP/1394 group; some
parts reflect rough consensus achieved at the 41st IETF meeting in Los
Angeles, other parts reflect the editor’s distillation of comments on
the reflector since then and still other parts are new contributions to
the evolution of MCAP. Until subsequent revisions of this document are
posted that more clearly identify agreed areas, the reader should
consider this a work in progress very much subject to revision. This
document is not yet adopted by the IP/1394 working group.

2. DEFINITIONS AND NOTATION

2.1 Conformance

When used in this document, the keywords "may", "optional",
"recommended", "required", "shall" and "should" differentiate levels of
requirements and optionality and are to be interpreted as described in
RFC 2119.

Several additional keywords are employed, as follows:

expected: A keyword used to describe the behavior of the hardware or
software in the design models assumed by this standard. Other hardware
and software design models may also be implemented.

Internet-Draft 00 1394 MCAP April 1998
ignored: A keyword that describes bits, octets, quadlets or fields whose
values are not checked by the recipient.

reserved: A keyword used to describe objects---bits, octets, quadlets
and fields---or the code values assigned to these objects in cases where
either the object or the code value is set aside for future
standardization. Usage and interpretation may be specified by future
extensions to this or other standards. A reserved object shall be zeroed
or, upon development of a future standard, set to a value specified by
such a standard. The recipient of a reserved object shall not check its
value. The recipient of an object defined by this standard as other than
reserved shall check its value and reject reserved code values.

2.2 Glossary

The following terms are used in this standard:

bus ID: A 10-bit number that uniquely identifies a particular bus within
a group of multiple interconnected buses. The bus ID is the most
significant portion of a node’s 16-bit node ID. The value 0x3FF
designates the local bus; a node shall respond to requests addressed to
its 6-bit physical ID if the bus ID in the request is either 0x3FF or
the bus ID explicitly assigned to the node.

IP datagram: An Internet message that conforms to the format specified
by RFC 791.

node ID: A 16-bit number that uniquely identifies a Serial Bus node
within a group of multiple interconnected buses. The most significant 10
bits are the bus ID and the least significant 6 bits are the physical

ID.

octet: Eight bits of data.

packet: Any of the 1394 primary packets; these may be read, write or
lock requests (and their responses) or stream data. The term "packet" is
used consistently to differentiate 1394 packets from ARP
requests/responses or IP datagrams.

physical ID: On a particular bus, this 6-bit number is dynamically
assigned during the self-identification process and uniquely identifies
a node on that bus.

quadlet: Four octets, or 32 bits, of data.

stream packet: A 1394 primary packet with a transaction code of 0x0A
that contains a block data payload. Stream packets may be either
asynchronous or isochronous according to the type of 1394 arbitration
employed.

2.3 Abbreviations

The following are abbreviations that are used in this standard:

Internet-Draft 00 1394 MCAP April 1998

   CAM Channel allocation manager
   MCAP Multicast channel allocation protocol
   IP Internet protocol (within the context of this document, IPv4)

3. CHANNEL ALLOCATION MANAGER

MCAP requires the presence of a channel allocation manager (CAM) to
process requests, allocate or deallocate Serial Bus channel numbers and
advertise the mapping from group addresses to their corresponding
channels.

The identity of the CAM and the method of its selection have not yet
been discussed by the working group.

Consensus has been reached that the CAM listens for messages (whose
format is described below) on the default multicast channel specified by
the NETWORK_CHANNELS register and transmits advertisements and other
responses on the same channel. The details of CAM operations are
described in section 5.

4. MCAP MESSAGE FORMAT

MCAP messages, whether sent by a multicast source or recipient or the
CAM, share a common format illustrated below. The first eight octets of
the message are fixed; the remainder consists of variable-length tuples,
each of which encodes information about a particular multicast group.

                        1                   2                   3
    0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1
   +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
   |             length            |            checksum           |
   +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
   |        bus_ID       |         reserved        |     opcode    |
   +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
   |                                                               |
   +                          message data                         +
   |                                                               |
   +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

                     Figure 5 - MCAP message format

Field usage in an MCAP message is as follows:

   length: This field shall contain the size, in octets, of the entire
   MCAP message.

   checksum: This field shall contain a checksum calculated on the
   entire MCAP message. The checksum shall be one’s complement of the
   sum of all the 16-bit words in the message; arithmetic overflow is
   discarded. For the purpose of calculating the checksum, the checksum
   field is treated as if zero.

Internet-Draft 00 1394 MCAP April 1998

   bus_ID: This field shall specify the 10-bit bus ID for which

   information in the MCAP message is valid. The value of bus_ID shall

   be equal to the most significant 10 bits of the sender’s NODE_IDS

   register.

   opcode: This field shall have one of the values specified by table 1

   below.

                      Table 1 - MCAP opcode values

    opcode    Name      Comment

   +----------------------------------------------------------------+

   |   0   | Advertise | Sent by the CAM to broadcast the current   |

   |       |           | mapping from each group address to its     |

   |       |           | corresponding channel number.              |

   |   1   |  Request  | Sent by a multicast source to request the  |

   |       |           | allocation of a channel number or to       |

   |       |           | refresh the remaining lifetime of a        |

   |       |           | channel number allocation.                 |

   |   2   |  Release  | Optionally sent by a multicast source to   |

   |       |           | release a channel number at a future time. |

   |   3   |   Error   | Sent by the CAM when it is unable to       |

   |       |           | satisfy a channel number allocation        |

   |       |           | request.                                   |

   |   4   |  Solicit  | Sent to request the CAM advertise the      |

   |       |           | current channel mapping(s) as soon as      |

   |       |           | possible.                                  |

   +----------------------------------------------------------------+

   message data: The remainder of the MCAP message is variable in length

   and shall consist of zero or more group address descriptors with the

   format illustrated below.

                        1                   2                   3

    0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1

   +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

   |     length    |      type     |            reserved           |

   +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

   |   expiration  |    channel    |     speed     |     status    |

   +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

   |                           bandwidth                           |

   +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

   |                                                               |

   +                         group_address                         +

   |                                                               |

   +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

            Figure 5 - MCAP group address descriptor format

   length: This field shall contain the size, in octets, of the MCAP

   group address descriptor.

Internet-Draft 00 1394 MCAP April 1998

   type: This field shall have a value of one, which indicates a group
   address descriptor.

   expiration: The usage of this field varies according to opcode. For
   solicit and error messages the expiration field shall be ignored.
   Otherwise this field shall contain a time-stamp, in seconds, that
   specifies a future time for the release of the channel number
   specified by channel. Time is expressed in terms of the
   CYCLE_TIME.seconds and a match occurs when expiration equals the most
   significant seven bits of the CYCLE_TIME register.

   channel: This field shall specify either a valid channel number, in
   the range zero to 63 inclusive, or else indicate an invalid channel
   number with a value of 0xFF. All other values are reserved. The usage
   of this field varies according to opcode, as shown in the table
   below.

              Operation   Usage of channel
            +----------------------------------------------+
            | Advertise | Channel number allocated for the |
            |           | multicast group_address          |
            |  Request  | Suggested channel number (hint)  |
            |  Release  | Ignored                          |
            |   Error   | Ignored                          |
            |  Solicit  | Ignored                          |
            +----------------------------------------------+

   speed: This field shall be ignored except for advertise and request
   messages, in which case it shall specify the speed at which stream
   packets for the indicated channel are transmitted. The encoding used
   for speed is specified by the table below; all values not specified
   are reserved.

                              Value   Speed
                            +---------------+
                            |   0   |  S100 |
                            |   1   |  S200 |
                            |   2   |  S400 |
                            |   3   |  S800 |
                            |   4   | S1600 |
                            |   5   | S3200 |
                            +---------------+

   status: This field shall be ignored except for error messages, in
   which case it shall characterize the reason(s) the CAM did not
   allocate a requested channel number. The encoding for this field is
   yet to be determined.

   bandwidth: This field shall be ignored; it is allocated in the group
   address descriptor to accommodate future extensions to MCAP that
   specify quality of service and utilize the isochronous capabilities
   of Serial Bus.

Internet-Draft 00 1394 MCAP April 1998

   group_address: This variable length field shall specify the IP

   address of a particular multicast group. The length of group_address,

   in octets, is derived from the length of the group address descriptor

   by subtracting 12 from the length field.

5. MCAP OPERATIONS

MCAP is a cooperative protocol implemented by multicast senders and
recipients and the CAM. The participants exchange messages over the
default multicast channel used by all IP-capable nodes on a particular

Serial Bus.

The bus_ID field in all MCAP messages shall be equal to the most
significant 10 bits of the sender’s NODE_IDS register.

5.1 Advertisement of channel mappings

The CAM shall periodically broadcast an advertisement of all multicast
group addresses allocated a channel number that differs from the default
multicast channel number. An advertisement shall consist of a single

MCAP message with an opcode of zero which contains zero or more group
address descriptors (one for each group address assigned a channel
number other than that specified by the NETWORK_CHANNELS register).

Within each group address descriptor, the group_address and channel
fields associate a multicast group address with a Serial Bus channel
number. More than one multicast group address may be mapped to a single

Serial Bus channel number by means of separate group address
descriptors. The speed field specifies the maximum 1394 speed at which
any of the senders within the multicast group transmits data. The
expiration field specifies a future time when the CAM will deallocate
the channel number.

No more than ten seconds shall elapse from the transmission of the most
recent advertisement before the CAM initiates transmission of the
subsequent advertisement.

5.2 Request for channel allocation

Before any multicast transmission on other than the default channel
number specified by the NETWORK_CHANNELS register, a sender within a
multicast group shall insure that the CAM has allocated a channel
number.

A multicast sender should first listen for an MCAP advertisement. If the
multicast group address is already mapped to a channel number, the
sender need not make a channel allocation request and may use the
advertised channel number for multicast transmission.

Otherwise the intended multicast sender shall transmit an MCAP message
with an opcode of one which contains one or more group address
descriptors. Within each group address descriptor the group_address
field shall specify the multicast group address for which a channel

Internet-Draft 00 1394 MCAP April 1998
the nature of the error. All other fields within the group address
descriptor shall be ignored.

5.4 Release of unneeded channel(s)

When a multicast sender intends to cease transmissions for a multicast
group that is not mapped to the default multicast channel, it may notify
the CAM by means of an MCAP release message. The usage of the release
message is optional, since the CAM will automatically deallocate the
channel number when its expiration time is reached.

An MCAP release message has an opcode value of three and contains one or
more group address descriptors. Each descriptor identifies the
group_address whose channel number is to be released. The expiration
field shall specify a time at least 30 seconds in the future for the
release of the channel number. All other fields within the group address
descriptor shall be ignored.

In response to an MCAP release message that identifies a group_address
in the current channel map, the CAM shall update the expiration time for
the channel with the value of expiration and shall transmit an MCAP
advertisement message as soon as possible. The advertisement that
reflects the updated expiration time is the response expected by the
sender of the MCAP release message.

Whether multicast senders utilize the optional MCAP release message or
not, channel allocations eventually expire for unused channel numbers.

When the expiration time associated with a particular multicast group
and associated channel is reached (as measured by the CAM’s CYCLE_TIME
register), the CAM shall remove the multicast group and channel number
from the current channel map. Once the CAM has transmitted an MCAP
advertisement message in which no group descriptors reference a
previously allocated channel number, the CAM shall deallocate the
channel number in the isochronous resource manager’s CHANNELS_AVAILABLE
register.

5.5 Solicitation of the channel map

Multicast recipients or senders may request the CAM to advertise the
channel map by transmitting an MCAP solicitation request. No group
address descriptors are included with this message; the opcode value of
five requests the CAM identified by bus_ID to advertise the channel map.

Originators of MCAP solicitation requests shall limit the rate at which
they are transmitted. Subsequent to sending a solicitation request,
neither the originator nor any other node that observes the request
shall send another MCAP solicitation request until either a) 10 seconds
have expired or b) an MCAP advertisement has been observed.

The CAM should transmit an MCAP advertisement message as soon as
possible in response to the solicitation request.

Internet-Draft 00 1394 MCAP April 1998

Expires: October, 1998 [Page 11]

5.6 Periodic refresh of channel allocation(s)

As described in 5.4 above, the CAM shall remove expired multicast group
address and channel number pairs from the current channel map and
ultimately return channel number(s) to the CHANNELS_AVAILABLE pool when
no longer used by any multicast group.

In order to prevent this occurrence for active multicast groups, at
least one sender within a multicast group shall periodically extend the
expiration time for the channel map by means of an MCAP channel
allocation request message (see 5.1). Although the CAM does not allocate
a new channel, the request causes the expiration time to be updated to a
new future value. The frequency of MCAP channel allocation request
messages and the expiration time specified in each should be coordinated
such that at least three request messages are transmitted before the
expiration time specified by the earliest of the three is reached.

In multicast groups where there is more than one sender it is desirable
to limit the number of MCAP channel allocation request messages. The
ideal situation is for one sender to generate the requests. If this
sender intends to leave the multicast group, one of two events occur:
either the sender transmits the optional MCAP release message or it
ceases transmission of allocation request messages. In the first case,
one of the other senders within the multicast group is expected to
observe the release message and initiate its own transmission of MCAP
channel allocation request messages. Otherwise, if the time remaining
before channel expiration falls below two seconds, that sender should
initiate its own transmission of MCAP channel allocation request
messages. In the latter case, the allocation request shall be
transmitted at least one second before the expiration time.

6. SECURITY CONSIDERATIONS

This document specifies the use of an unsecured link layer, Serial Bus,
for the transport of IPv4 datagrams. Serial Bus is vulnerable to denial
of service attacks; it is also possible for devices to eavesdrop on data
or present forged identities. Implementers who utilize Serial Bus for
IPv4 should consider appropriate counter-measures within application or
other layers.

7. ACKNOWLEDGEMENTS

This document represents work in progress by the IP/1394 Working Group.
The editor wishes to acknowledge the contributions made by all the
active participants, either on the reflector or at face-to-face
meetings, which have advanced the technical content.

8. REFERENCES

[1] IEEE Std 1394-1995, Standard for a High Performance Serial Bus

[2] ISO/IEC 13213:1994, Control and Status Register (CSR) Architecture
    for Microcomputer Buses

Internet-Draft 00 1394 MCAP April 1998

[3] IEEE Project P1394a, Draft Standard for a High Performance Serial

    Bus (Supplement)

[4] IEEE Project P1394b, Draft Standard for a High Performance Serial

    Bus (Supplement)

9. EDITOR�S ADDRESS

Peter Johansson

Congruent Software, Inc.

3998 Whittle Avenue

Oakland, CA  94602

(510) 531-5472

(510) 531-2942 FAX
pjohansson@aol.com